[NEXT-PSE4809AT]

모델명	NEXT-PSE4809AT
Item	Description
No. of channels	1
Pass Through Data Rates	10/100/1000 Mbps
Power over Ethernet Output	Pin Assignment and Polarity: 1/2(-), 3/6(+) Ourput Power Voltage: 54V User Port Power: 30W max
Input Power Reauierements	Ac Input Voltage: 100 to 240V AC Input Current: 0.5A 100-240V AV Frequency: 50 to 60Hz
Dimension	118mm x 48mm x 34mm
Indicators	System Indicator: AC Power User Indicator: Channel Power
Connectors	Shielded RJ-45, EIA 568A and 568B
Protection	Over current protection Over load protection Over voltage protection Anti-interfernce protection
Environmental Conditions	Operating Ambient Temperature 0 to 40℃ Operating Humidity: Maxium 90%, Non-condensing Storage Temperature: -40 to 70℃ Storage Humidity: Maxium 90%, Non-condensing
Regulatory Comliance	IEEE 802.3af(PoE) / IEEE 802.3at(PoE+)