[NEXT-POE4807J-60W]

모델명	NEXT-POE4807J-60W
Item	Description
No. of channels	1
Pass Through Data Rates	10/100/1000 Mbps
Power over Ethernet Output	1/2(-), 3/6(+), 4/5(+), 7/8(-) Ourput Power Voltage: 50V User Port Power: 30W & 60W
Input Power Reauierements	Ac Input Voltage: 100 to 240V AC Input Current: 0.5A 100-240V AV Frequency: 50 to 60Hz
Dimension	168mm x 73.5mm x 44mm
Indicators	System Indicator: AC Power User Indicator: Channel Power
Connectors	Shielded RJ-45, EIA 568A and 568B
Protection	Over current protection Over load protection Over voltage protection Anti-interfernce protection
Environmental Conditions	Operating Ambient Temperature 0 to 40℃ Operating Humidity: Maxium 85%, Non-condensing Storage Temperature: -10 to 50℃ Storage Humidity: Maxium 90%, Non-condensing