[NEXT-POE910F-2TP]

모델명	NEXT-POE910F-2TP
Item	Description
Networt Port	8 10/100Mbps PoE RJ45 port (port 1~8) 2 10/100Mbps non-PoE RJ45 port (port 9~10)
Pass Through Data Rates	100Mbps full duplex
Standard SPEC.	IEEE802.3i, IEEE802.3u, IEEE802.3x, IEEE802.3ab, IEEE802.3af, IEEE802.3at
Performance	Bandwidth: 2.0Gbps(no Block) Frame filtering and transmission rate: 10M port maximum 14,800pps 100M port maximum 148,800pps
LED Indicator	Power/Link/ACT/RESV/POE Indicator light
PoE Pin	1/2+, 3/6-
Power Requirements	Max. output power single port: 30W Internal Power supply: 96W
Size	210mm x 40mm x 152mm
Weight	1.5kg
Environmetal Conditions	Operating Temperature: 0~40℃ Operating Humidity:１０～９０％
Safety Certification	CE/ROHS/FCC/KC